1x Annulus
1x Front
3x Hook mechanism
1x Knob
1x Shuttle

You'll also need the following hardware items:
5x 608Z or 608ZZ bearing (A standard 22mm OD, 8mm ID, 7mm high) amazon.com
2x M8 machine bolt 
2x M8 lock nut 
3x M8 washers


Assembly Instructions. Insert Bearings into Front part they only go in one way and there are 4 total.
Insert the bearing into the Radial gear it also only goes in one way 
Install the hooks through the front and Install the gears onto the Hooks then insert 
the little lock into the hook to lock it to the gear.
Install 1 M8 nut into the Knob install one of the M8 Bolts through the Bearing in the 
radial gear and thread the Knob onto it and tighten.
Install the last M8 Bolt into the Radial gear in the hex slot push it all the way in 
install 2 washers onto the bolt and install the assembly onto the from part over 
The gears
Install the last washer then the nut and tighten. Mount to a table or your bench 
and have at it.

You May not sell this design under any circumstances, you are free to build and use it 